QNX2-TCP/IP
-----------

(c) Andre Koppel Software 1996-1998
(c) SW Datentechnik 1996-1998


This archiv contains a demo-version of our TCP/IP-package for QNX2.
The software runs with allmost every NE2000-compatible ISA-card.
This archiv also contains the free program rawrite3.com, that is
used to copy the raw disk-images to a QNX2-disk. Also contained within
this archiv you will find the manual as a Adobe Acrobat PDF-file.

Installation
------------

Preformat two QNX2-disks:

        fdformat 1 +1.4meg

Use the dos-utility (which runs fine under Win95) to generate a QNX2-
archiv disk. Enter "rawrite3" at the command-prompt (or press the right
mouse-button on the Win95-Startbutton and select open). The rawrite3-
utility asks for a file-name. Enter "q2tcpd1.raw" and press enter. Then
rawrite3 asks for a destination-diskdrive. Normally you must enter A for
your 3,5" drive. Insert the first of the two preformated QNX2-disks and
press enter. The rawrite3-utility then generates the first QNX2-disk
containing the TCP/IP-package. Repeat the steps to generate the second
disk.

Start your QNX2-computer and enter the following on the command-prompt:

        backup 1:/ 3:/ +all -p l=10

This copies all the files from one disk to you harddisk. Repeat the backup
for the second disk.

Run the setup-program:

        /etc/setup

To run the demoversion you need a temopary-license-code which may be obtained
from SW Datentechnik (via E-Mail, FAX or phone). The license code consists
of 24 alphanumeric-characters stored in the file /etc/akstcp.sercode.

After you have installed the package and entered the license-code you must
enter the base-I/O-adress and the IRQ used by your NE2000-card. This is
done within the file /etc/rc.d/rc.inet1.

For additional information how to install and configure the software please
read the manual.

        Good look

